# forceMvccCheckpoint {#forceMvccCheckpoint}

**Parent topic:**[Functions](../../Functions/category.md)

## Syntax {#topic_e5g_35w_3zb}

`forceMvccCheckpoint(mvccTable)`

## Arguments {#topic_f5g_35w_3zb}

**mvccTable** is the handle of the MVCC table. To obtain a handle of a persisted MVCC table, you can call function `loadMvccTable`.

## Details {#topic_g5g_35w_3zb}

Manually trigger a checkpoint for the specified MVCC table and clear the data in the log.

